TVMR2|$25f800000
VDP2EXT|$25f800002
SCRSTATE|$25f800004
VRAMSIZE|$25f800006
VDP2RAMCR|$25f80000E
BGREG|$25f800020
MOZAIC|$25f800022|Mosaic Control Register
VDP2CCRA|$25f800028|Character Control Register
VDP2CCRB|$25f80002A
VDP2BMPAL|$25f80002C|Bit Map Palette Number (NBG0, NBG1)

BG0PATTERN|$25f800030
BG1PATTERN|$25f800032

MAPOFFR|$25f80003C

BG0SCROLLHI|$25f800070|NBG0 horizontal direction (integer part)
BG0SCROLLHF|$25f800072|NBG0 horizontal direction (fractional part)
BG0SCROLLVI|$25f800074|NBG0 vertical direction (integer part)
BG0SCROLLVF|$25f800076|NBG0 vertical direction (fractional part)

BG1SCROLLHI|$25f800080|NBG1 horizontal direction (integer part)
BG1SCROLLHF|$25f800082|NBG1 horizontal direction (fractional part)
BG1SCROLLVI|$25f800084|NBG1 vertical direction (integer part)
$25f800086|NBG1 vertical direction (fractional part)

BGDZOOM|$25f800098|reduction enable register

BGVPOSINCR|$25f80009A
SPPRIORITY|$25f8000EA
BGPRIORITY|$25f8000F8